# Adafruit STMPE610 Library [![Build Status](https://github.com/adafruit/Adafruit_STMPE610/workflows/Arduino%20Library%20CI/badge.svg)](https://github.com/adafruit/Adafruit_STMPE610/actions)[![Documentation](https://github.com/adafruit/ci-arduino/blob/master/assets/doxygen_badge.svg)](http://adafruit.github.io/Adafruit_STMPE610/html/index.html)

<a href="http://www.adafruit.com/products/1571"><img src="assets/board.jpg?raw=true" width="500px"></a>

This is a library for the Adafruit STMPE610 Resistive
touch screen controller breakout
* http://www.adafruit.com/products/1571

Check out the links above for our tutorials and wiring diagrams
These breakouts use SPI or I2C to communicate

Adafruit invests time and resources providing this open source code,
please support Adafruit and open-source hardware by purchasing
products from Adafruit!

Written by Limor Fried/Ladyada for Adafruit Industries.
MIT license, all text above must be included in any redistribution

To install, use the Arduino Library Manager and search for "Adafruit STMPE610" and install the library.

